======================================================================================
Model Parameters
======================================================================================
26                        : Number of parameters in this section
SimLab                    : EFlo GUI name
2021.2                    : EFlo GUI version [EFLOGVER]
2021.2                    : EFlo Solver version
0                         : Flag for SD [FLGSD]
0                         : Flag for Restart option [FLGRST]
500                       : Max overal solver iteration [PRTSTP]
0                         : Display flag (0: no "Close Window?" message)[Pg_DspFlg]
500                       : Max number of iterations (Overall) [MNITLP]
500                       : Max number of iterations (Flow) [MNIFL]
900                       : Max number of iterations (Field Solver) [ICR11]
1                         : Switch for generating log file [SWDLOG]
0                         : Not-used [SWSSCONV]
0                         : -        [NCRRPASS]
0                         : Switch for Post-Processing only [SWPOST] 
0                         : Switch for non-CFD (1: Non-CFD, 0: Full-CFD) [SWNCFD]
0                         : Switch for including electrical simulation [SWELECT]
1                         : Electrical Parameter: [ISTVOLT]
5                         : Electrical Parameter: [TMXVOLT]
0                         : Flag to detect circuits, write output and exit
0                         : Flag to read restart file, dump fields and exit
0                         : Flag to generate QA file
1                         : Verbosity level
173.15                    : Min acceptable temperature (stop simulation if lower)
1.07315000e+03            : Max acceptable temperature (stop simulation if higher)
-100.0                    : Min acceptable velocity (stop simulation if lower)
100.0                     : Max acceptable velocity (stop simulation if higher)
0                         : N/A
0                         : N/A
0                         : N/A
0                         : N/A
0                         : N/A
0                         : N/A
0                         : N/A



======================================================================================
Solver Parameters
======================================================================================
12                        : Number of parameters in this section
0.00000000e+00            : Starting time [TMSTRT]
1.00000000e+00            : Time step [DTIME]
7.50000000e-02            : Time step 2 [DTIME2]
2.93150000e+02            : Reference temperature (Ambient/Initial temperature) [TRF]
5.00000000e-06            : Not-used (Tolss) [TOLSS]
1.00000000e-03            : Thermal convergence metric [TOLTR]
1.00000000e-02            : CFD convergence metric [TOLFL]
5.00000000e-05            : Temperature equation solver tolerance [TOLT]
5.00000000e-04            : Pressure equation solver tolerance [TOLP]
1.00000000e-04            : Velocity equation solver tolerance [TOLUR]
5.00000000e-04            : Pressure-correction equation solver tolerance [TOLVCP]
0.00000000e+00            : Reference Voltage [VOLTRF]
1                         : Use fast matrix solver for momentum
0                         : Sensor ID for thermal convergence
0                         : Sensor type (1: Average, 2: Max, 3: RMSE)
0                         : N/A
0                         : N/A
0                         : N/A
0                         : N/A



======================================================================================
Transient Parameters
======================================================================================
1                         : Number of parameters in this section
1000                      : Switch for Steady-State (non-zero:steady-state,0:Transient)[SWSSS]



======================================================================================
Output Parameters (for each: Flag, multiplication factor, offfset factor, unit)
======================================================================================
23       : Number of parameters in this section
22       : Number of output parameters
1        : Length
3        : Temperature
3        : Velocity
3        : Pressure
0        : Voltage
0        : Power
0        : Turb.K
0        : Turb.Eps
0        : Turb.Mu
0        : Conductivity
0        : Mass Source
0        : Transient Err
0        : Circuit-ID
3        : Joule-heating
0        : Current-Density
0        : Part-max-temperature
0        : Part-thermal-margines
0        : Case-temperatures
0        : Board-temperatures
0        : CFL
0        : Elemental Transient metrics (thermal)
0        : Elemental Transient metrics (CFD)



======================================================================================
Gravity
======================================================================================
4                        : Number of parameters in this section
9.81000000e+00           : Magnitude
0.00000000e+00           : Vector component in x-dir
0.00000000e+00           : Vector component in y-dir
-1.00000000e+00           : Vector component in z-dir



======================================================================================
Turbulence Parameters
======================================================================================
7                        : Number of parameters in this section
4                        : Switch for turbulence modeling [SWTRB]
8.50000000e-01           : Prandtl_Turb[KE_PrT]
1.00000000e-02           : distance-to-wall cap
1.00000000e+02           : viscosity-ratio cap
0                        : N/A
0                        : N/A
0                        : N/A



