Linear Static Step

Problem submitted Mon Nov 19 15:04:46 2018
Input file C:/Users/vbgundepudi/Documents/Tutorials/FEM_OS/Parametric Optimization/Simulation/fan_Solution.fem

Problem summary

- Problem parameters: C:/Users/vbgundepudi/Documents/Tutorials/FEM_OS/Parametric Optimization/Simulation/fan_Solution.fem
- Finite element model: C:/Users/vbgundepudi/Documents/Tutorials/FEM_OS/Parametric Optimization/Simulation/fan_Solution.fem
- Output files prefix: fan_Solution

- Finite element model information

  Number of nodes: | 15085
  Number of elements: | 7250
  Number of degrees of freedom: | 44787
  Number of non-zero stiffness terms: | 1518297

  - Elements

    Number of TET10 elements: | 7250

  - Loads and boundaries

    Number of FORCE sets: | 2
    Number of SPC sets: | 2

  - Materials and properties

    Number of PSOLID cards: | 1
    Number of MAT1 cards: | 1

- Subcases & loadcases information
  - Static subcases

    Subcase ID | SPC ID | Force ID | Weight
    1 | 4 | 3 | 1.00

  Results summary

  Click here to view the results with HyperViewPlayer. This feature requires a modern browser with Javascript enabled, as well as the HyperViewPlayer plugin installed.

- Subcase 1 -
  - Maximum displacement is 170. at grid 1435.
  - Maximum 3-D element stress is 0.197E+06 in element 8285.

  © 1996-2018 Altair Engineering, Inc.